# Release defaults: -Os, no console UART, BLE log via 0xFFE3
# Build: idf.py -DSDKCONFIG_DEFAULTS="sdkconfig.defaults;sdkconfig.defaults.release" build

# CONFIG_COMPILER_OPTIMIZATION_DEBUG is not set
CONFIG_COMPILER_OPTIMIZATION_SIZE=y
# CONFIG_COMPILER_OPTIMIZATION_DEFAULT is not set
# CONFIG_COMPILER_OPTIMIZATION_PERF is not set
# CONFIG_COMPILER_OPTIMIZATION_NONE is not set

# CONFIG_COMPILER_OPTIMIZATION_ASSERTIONS_ENABLE is not set
CONFIG_COMPILER_OPTIMIZATION_ASSERTIONS_SILENT=y
# CONFIG_COMPILER_OPTIMIZATION_ASSERTIONS_DISABLE is not set

# CONFIG_ESP_COREDUMP_ENABLE is not set

# CONFIG_LOG_DEFAULT_LEVEL_INFO is not set
CONFIG_LOG_DEFAULT_LEVEL_WARN=y
CONFIG_LOG_DEFAULT_LEVEL=2

# Release: no UART console (W/E via BLE 0xFFE3 notify)
# CONFIG_ESP_CONSOLE_UART_DEFAULT is not set
CONFIG_ESP_CONSOLE_NONE=y

# When APP_UART_MODE_DEBUG=y: uart_comm uses UART from APP_DEBUG_UART_*; no ESP_LOG

CONFIG_ROBO_APP_FW_RELEASE=y
# CONFIG_ROBO_APP_FW_DEBUG is not set

CONFIG_LOG_BOOTLOADER_LEVEL_WARN=y
CONFIG_LOG_BOOTLOADER_LEVEL=2

# CONFIG_BT_NIMBLE_LOG_LEVEL_INFO is not set
CONFIG_BT_NIMBLE_LOG_LEVEL_WARNING=y
CONFIG_BT_NIMBLE_LOG_LEVEL=2
